# 网络设备答题卡B卷

## VSU

|  |
| --- |
| BB-VSU-S6000#show switch virtual |
|  |
| BB-VSU-S6000#show switch virtual dual-active bfd |
|  |
| BB-VSU-S6000#show ip ospf neighbor |
|  |
| BB-VSU-S6000#show aggregatePort summary |
|  |
| BB-VSU-S6000#show ip inter brief |
|  |

## S3

|  |
| --- |
| GZFB-S5750-01#show vrrp brief |
|  |
| GZFB-S5750-01#show ipv6 interface brief |
|  |
| GZFB-S5750-01#show ipv6 vrrp brief |
|  |

## S4

|  |
| --- |
| GZFB-S5750-02#show ip ospf neighbor |
|  |
| GZFB-S5750-02#show ip ospf interface vlan 10 |
|  |

## S5

|  |
| --- |
| JLFB-S5750-01#show interface gigabitEthernet 0/1 | be Bridge attributes |
|  |

## S6

|  |
| --- |
| GZFB-S2910-1#show version |
|  |
| GZFB-S2910-1#show interface switchport | include TRUNK |
|  |
| GZFB-S2910-1#show run interface gigabitEthernet 0/13 |
|  |
| GZFB-S2910-1#show ip dhcp snooping |
|  |
| GZFB-S2910-1#show nfpp log summary |
|  |
| GZFB-S2910-1#show run interface gigabitEthernet 0/23 |
|  |
| GZFB-S2910-1#show cpu-protect cpu |
|  |
| GZFB-S2910-1#show spanning-tree summary |
|  |

## S7

|  |
| --- |
| BB-S2910-1#show run | in password |
|  |
| BB-S2910-1#show run | include snmp |
|  |

## R1

|  |
| --- |
| BB-RSR20-01#show ip route |
|  |
| BB-RSR20-01#show access-lists |
|  |
| BB-RSR20-01# show run | be ip nat pool (截取NAT相关配置) |
|  |

## R2

|  |
| --- |
| ISP-RSR20-01#show ip bgp summary |
|  |

## R3

|  |
| --- |
| ISP-RSR20-02#show run | include password 、ISP-RSR20-02#show run | begin line |
|  |
| ISP-RSR20-02#show bgp ipv4 unicast summary |
|  |
| ISP-RSR20-02#show rate-limit interface gigabitEthernet 0/0 |
|  |
| ISP-RSR20-02#show traffic-shape serial 3/0 |
|  |

## EG1

|  |
| --- |
| GZFB-EG2000-01#show ip route |
|  |
| GZFB-EG2000-01#show flow-control Gi0/3 |
|  |
| GZFB-EG2000-01#show content-policy |
|  |
| GZFB-EG2000-01#show url-class user-cfg |
|  |
| GZFB-EG2000-01#show run | begin ip nat pool |
|  |
| GZFB-EG2000-01#show crypto isakmp sa |
|  |
| GZFB-EG2000-01#show crypto ipsec sa | include #pkts decaps: |
|  |

## EG2

|  |
| --- |
| JLFB-EG2000-01#show ip route |
|  |
| JLFB-EG2000-01#show run | begin ip nat pool |
|  |
| JLFB-EG2000-01#show ip session filter |
|  |
| JLFB-EG2000-01#show access-lists |
|  |
| JLFB-EG2000-01#show crypto ipsec transform-set |
|  |
| JLFB-EG2000-01#show crypto map mymap |
|  |

## AC1

|  |
| --- |
| BB-WS6008-01#show wlan-config summary(无线用户关联成功后收集) |
|  |
| BB-WS6008-01#show ap-config summary |
|  |
| BB-WS6008-01#show wlan-config cb 1 |
|  |
| BB-WS6008-01#show ap-group intf-wlan-map GZ |
|  |
| BB-WS6008-01#show wlan hot-backup 11.1.0.22 |
|  |
| BB-WS6008-01#show wlan security 1 |
|  |
| BB-WS6008-02#show version all (截取GZFB-AP520-01版本信息) |
|  |

## AC2

|  |
| --- |
| BB-WS6008-02#show ap-group intf-wlan-map JL |
|  |
| BB-WS6008-02#show run | include wlan-based |
|  |
| BB-WS6008-02#show ap-config running |
|  |
| BB-WS6008-02#show schedule session |
|  |
| BB-WS6008-02#sh run | include disabled |
|  |
| BB-WS6008-02#show wids whitelist |
|  |
| BB-WS6008-02#show wlan hot-backup 11.1.0.21 |
|  |

## 验证测试

|  |
| --- |
| GZFB-S5750-01#ping 192.1.20.254 source 193.1.20.252 |
|  |
| JLFB-S5750-01#ping 192.1.20.254 source 194.1.20.254 |
|  |
| tracert 10.1.0.18 (PC1手动配置地址后) |
|  |
| Ipconfig （PC1使用无线网卡获取IPv4和IPv6地址） |
|  |
| PC1路径跟踪到192.1.120.254 tracert <192.1.20.254> |
|  |
| PC1获取IPv6地址后Ping 2001:193:40::254 |
|  |